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SwitchGroup1:




do

high 4, 7

pause 800

low 4, 7

inc b1

loop while b1 < 10

goto Main


SwitchGroup2:

do

high 6, 5 

pause 800  



low 6, 5

inc b1

loop while b1 < 10

goto Main


SwitchGroup3:

do

high 4, 7

pause 800

low 4, 7

pause 200

high 6, 5 

pause 800  



low 6, 5

pause 200

inc b1

loop while b1 < 10

goto Main
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Finishes loop


Exits low.








